**Block Device (TABU)**

Plugging systems Block Device (TABU)

are designed to shut off the pipeline

during repair work and tie-in work

without disconnecting consumers. The

equipment is mounted on valves and

is designed to be used in conjunction

with straight fittings and tee fittings.

Plugging system Block-Device (TABU)

are equipped with flange adapters for

mounting on valves and equipped with

outlets for organizing bypass lines.

The working element designed to seal

the pipe cavity is a cuff of trapezoidal

section, which is deformed by two plates

having inner tapered surfaces.

Depending on the size and operating

pressure of the pipeline, the equipment

can be equipped with a manual or hydromechanical

drive of plates and various

mechanisms for input / output of

blocking heads into the cavity of the

pipeline (manual or hydraulic).

Block-Device (TABU) can be equipped

with video surveillance points connected

to the video diagnostic system and

allowing to visually control the equipment

operation process in real time.

Power to the hydraulic drives of the

Block-Device (TABU) is carried out from

a hydraulic oil station with a working

pressure of 14.0 MPa and a flow rate of

30 l / min.

**Technical details of Block-Device (TABU) ОБСУДИТЬ!!!**

**Consumables for Plugging systems Block-Device (TABU)**

|  |  |  |  |
| --- | --- | --- | --- |
|  | Material | | Art. № |
| NBR | Polyurethane |
| Cuff 50 | х |  | TS0813 |
| Cuff 65 | х |  | TS0814 |
| Cuff 80 | х |  | TS0815 |
| Cuff 100 | х |  | TS0816 |
| Cuff 125 | х |  | TS0817 |
| Cuff 150 | х |  | TS0818 |
| Cuff 200 | х |  | TS0819 |
| Cuff 250 | х |  | TS0820 |
| Cuff 300 | х |  | TS0821 |
| Cuff 350 |  | х | TS0822 |
| Cuff 400 |  | х | TS0823 |
| Cuff 450 |  | х | TS0824 |
| Cuff 500 |  | х | TS0825 |
| Cuff 600 |  | х | TS0826 |
| Cuff 700 |  | х | TS0827 |
| Cuff 800 |  | х | TS0828 |